{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["1.视频监控系统"],"read":"whole","date_system":"1900"}

{"sheet":"1.视频监控系统","index":0,"n_rows":42,"n_cols":9,"rows_kept":42,"merged":[[0,0,0,8],[1,0,1,8],[17,0,17,8],[18,0,18,7],[19,1,19,2],[19,3,19,4],[20,1,20,2],[20,3,20,4],[21,1,21,2],[21,3,21,4],[22,1,22,2],[22,3,22,4],[23,1,23,2],[23,3,23,4],[24,1,24,2],[24,3,24,4],[25,1,25,2],[25,3,25,4],[26,1,26,2],[26,3,26,4],[27,0,27,8],[28,0,28,8],[29,1,29,2],[29,3,29,4],[30,1,30,2],[30,3,30,4],[30,8,34,8],[31,1,31,2],[31,3,31,4],[32,1,32,2],[32,3,32,4],[33,1,33,2],[33,3,33,4],[34,1,34,2],[34,3,34,4],[35,0,35,8],[36,0,36,8],[37,0,37,8],[40,0,40,8],[41,0,41,8]]}
["2021年度下学期自然科学系实验室安全改造项目报价表"]
["一、视频控制系统"]
["序号","名称","品牌","设备型号","参数备注","数量","单位","单价","合计"]
[1,"200万星光级红外高清筒型摄像机POE","海康威视","DS-2CD3T26WDV3-L\n (4mm镜头)","传感器类型：1/2.7”Progressive Scan CMOS\n照度：彩色：0.005Lux@（F1.2，AGC ON），0 Lux with Light\n镜头：4mm，水平视场角：81.6°[6mm(50°)，8mm(38.7°)，12mm(24.2°)可选]\n图像尺寸： 1920×108\n视频压缩标准：主码流：H.265/H.264，子码流：H.265/H.264/MJPEG\n通讯接口：1个RJ45 10M/100M自适应以太网口\n尺寸：产品：186.6*92.9*93.5mm\n包装：235*120*125mm",9,"支"]
[2,"枪机支架","专用","专用",null,9,"个"]
[3,"网线","海康威视","UTP5","海康DS-1LN5E-S/E原装线０.５",3,"箱"]
[4,"16路硬盘录像机","海康威视","DS-7916N-R4","1.5U标准机架式IP存储/嵌入式处理器/嵌入式软硬件设计/16路/256M接入/256M转发/4盘位/关键视频添加标签和加锁保护/断网续传/SMART 2.0/2个千兆以太网口",1,"台"]
[5,"监控数据硬盘","WD","6T","监控盘",2,"个"]
[6,"主机柜",null,"17U",null,1,"个"]
[7,"16口全千兆POE交换机","海康威视","DS-3E0518P-E","二层非网管全千兆POE交换机\n支持IEEE 802.3at/af\n支持IEEE 802.3、IEEE 802.3u、IEEE 802.3x、IEEE802.3ab、IEEE802.3z\n支持6 KV防浪涌（PoE口）\n支持PoE输出功率管理\n千兆网络接入设计\n线速转发、无阻塞设计\n存储转发交换方式\n坚固式高强度金属外壳\n无风扇设计，高可靠性",1,"台"]
[8,"监控用监视器","AOC","LE43M3776普通","证书编号：2018010808059970证书状态：有效产品名称：液晶电视3C规格型号：LE43M3776、LE43M3778、T4376M、LE43M3775、T4376MA、 T437...产品名称：AOC AOC LE43M3776型号: LE43M3776品牌: AOC冠捷型号: AOC LE43M3776成色: 全新产地: 中国大陆屏幕比例: 16:9接口类型: HDMI面板类型: IPS-ADS颜色分类: 黑色套餐类型: 官方标配生产企业: 福建捷联电子有限公司能效等级: 二级附加功能: 可壁挂 内置音箱刷新率: 60Hz屏幕类型: LED屏幕分辨率: 1920*1080（全高清）屏幕尺寸: 43英寸",1,"台"]
[9,"3m HDMI 2.0视频连接线","绿联","绿联","支持4K画质输出，镀金接口防锈",1,"条"]
[10,"PVC管","联塑","φ25",null,60,"米"]
[11,"PVC管","联塑","φ20",null,180,"米"]
[12,"插线板","公牛","6插",null,1,"个"]
[13,"辅助材料",{"$nulls":3},1,"项"]
[14,"安装人工费",{"$nulls":3},1,"项"]
["小计：    元（人民币 万 仟 佰 拾 元 ）"]
["二、废液保管室设备"]
["序号","名称",null,"规格",null,"数量","单价","金额","备注"]
[1,"药箱",null,"12寸箱内含：烫伤膏1支，风油精1支，酒精片20片，碘伏片10片，灭菌纱布块2片，速冷冰袋1个，创可贴1盒，体温计1支，镊子1支，剪刀1把，PBT弹力绷带2个，无纺布胶带1个，绷带3个，止血带1个，棉签5包，急救手册1本，急救毯1条\n外带支架",null,"1个",null,null,"含支架安装"]
[2,"易燃易爆气体报警器",null,"1.含探头及控制显示器\n2.防爆风机：0.18kw，管道防爆轴流风机\n3.信号线：连接探头与控制显示器用\n4.地线铺设",null,"1套",null,null,"含安装，保质一年"]
[3,"锁头",null,"双胆锁 50MM 双钥匙开",null,"1个"]
[4,"警示标签",null,"定制",null,"10张"]
[5,"警戒线",null,"50米",null,"1卷"]
[6,"塑料方盘",null,"30*30*5cm  耐酸碱",null,"10个"]
[7,"人体静电释放器",null,"声光防爆报警款  高110cm\n（含地线铺设等费用）",null,"4个",null,null,"含安装，保质一年"]
["小计：    元（人民币 万 仟 佰 拾 元 ）"]
["三、倒L型定制挡板"]
["序号","名称",null,"型号规格",null,"数量","单价","合计","备注"]
[1,"倒L型定制挡板",null,"上板：2000mm*450mm\n下板：2000mm*100mm",null,"2套",null,null,"由一块上板和一块下板组成，材质为实芯理化板，厚度12.7mm"]
[2,"倒L型定制挡板",null,"上板：2000mm*460mm\n下板：2000mm*100mm",null,"2套"]
[3,"倒L型定制挡板",null,"上板：2000mm*470mm\n下板：2000mm*100mm",null,"2套"]
[4,"倒L型定制挡板",null,"上板：2000mm*530mm\n下板：2000mm*100mm",null,"1套"]
[5,"倒L型定制挡板",null,"上板：1010mm*520mm\n下板：1010mm*100mm",null,"1套"]
["注：★为保证实芯理化板材料质量以及从环保角度保障实验室人员健康，实芯理化板必须符合以下技术参数及要求：\n1.通过“国家化学建筑材料测试中心”检测，参与竞标的厂商所提供的台面材料需通过“国家化学建筑材料测试中心”的检测，并在竞标文件中提供相应检测报告复印件加盖生产厂家公章；\n2.通过“国家化学建筑材料测试中心”检测，参与竞标的厂商需在竞标文件中提供相应检测报告复印件并加盖生产厂家公章；\n3.通过“国家化学建筑材料测试中心”检测，按照GB/T 2406.2-2009检测，检测项目有氧指数判定合格，UL 94:2013水平燃烧，UL94:2013垂直燃烧，符合UL 94:2013燃烧测试规定的V-0的等级。\n\n"]
["小计：     元（人民币 万 仟 佰 拾 元 ）"]
["四、腐蚀品储存柜"]
["序号","名称",null,null,"规格","数量","单价（元）","金额（元）","备注"]
[1,"腐蚀品储存柜",null,null,"1800*900*450（高*长*宽/毫米）  PP材质 ","1台",null,null,"含安装及材料费"]
["小计：     元（人民币 万 仟 佰 拾 元 ）"]
["四项合计：      元（人民币 万 仟 佰 拾 元 ）(此报价含税含安装调试）"]